{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"images":41},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":72,"n_cols":9,"rows_kept":72,"merged":[[0,0,1,8],[3,0,13,0],[14,0,69,0],[14,1,30,1],[31,1,40,1],[41,1,50,1],[51,1,60,1],[61,1,69,1],[70,0,71,0],[70,1,71,1]]}
["第三人民医院楼层标识牌清单"]
[]
[null,null,"序号","类名","数量","尺寸cm","材质及工艺",null,"备注"]
["户外",null,1,"医院名称标识",6,"单字120","不锈钢字烤漆",null,"1.5MM厚304不锈钢围边字，精抛光，汽车喷漆红色，钢结构固定，吊车安装，侧厚10CM"]
[null,null,2,"医院总平图",1,"180*140","落地不锈钢造型牌",null,"2MM304不锈钢激光切割，焊接造型，精工打磨，表面汽车烤漆工艺，总平图UV平喷，内容丝网印刷,总厚度35CM"]
[null,null,3,"单体建筑名称标识",6,"单字80","不锈钢字烤漆及钢结构",null,"1.5MM厚304不锈钢围边字，表面5MM红色亚克力透光板，内置LED光源，发红色光，背面焊40*40*1.5MM不锈钢焊接框架,字总厚度5CM"]
[null,null,4,"道路及各单体建筑指向标识",2,"30*185","落地不锈钢造型牌",null,"1.5MM304不锈钢激光切割，焊接造型，内部镀锌管焊接框架，精工打磨，表面汽车烤漆，内容丝网印刷,总厚度10CM"]
[null,null,5,"急救通道标识",1,"34*40","烤漆、不锈钢牌",null,"1.5MM304不锈钢激光切割，焊接造型，精工打磨，表面汽车烤漆，内容丝网印刷,总厚度2CM"]
[null,null,6,"无障碍通道标识",1,"34*40","烤漆、不锈钢牌",null,"1.5MM304不锈钢激光切割，焊接造型，精工打磨，表面汽车烤漆，内容丝网印刷,厚2CM"]
[null,null,7,"花草牌",5,"40*60","不锈钢牌、预埋",null,"1.5MM304不锈钢激光切割，焊接造型，内部镀锌管焊接框架，精工打磨，表面汽车烤漆，内容丝网印刷，厚40CM"]
[null,null,8,"停车场导向牌",2,"55*120","落地不锈钢造型牌",null,"1.5MM304不锈钢激光切割，焊接造型，厚15cm,内部镀锌管焊接框架，精工打磨，表面汽车烤漆，内容丝网印刷，总厚度10CM"]
[null,null,9,"停车场标识牌",5,"35*40","落地不锈钢造型牌",null,"1.5MM304不锈钢激光切割，焊接造型，厚2cm,精工打磨，表面汽车烤漆，内容丝网印刷，总厚度2CM"]
[null,null,10,"车位、专用车位标识",10,"40*150","刷漆",null,"常温标线漆，5mmPVC板雕刻字模，"]
[null,null,11,"户外宣传公告栏",2,"320*220","落地不锈钢造型",null,"1.5MM304不锈钢激光切割，焊接造型，内部镀锌管焊接框架，精工打磨，表面汽车烤漆，内容丝网印刷，玻璃橱窗，内容画面可更换，雨棚宽65CM，架子厚10CM，基础预埋件"]
["户内","一楼",1,"玻璃门防撞条",20,"90*12","磨砂膜UV",null,"磨砂膜UV打印"]
[null,null,2,"告示架",2,"80*180","铝合金展架",null,"铝合金展示架，画面可更换（户外写真UV打印）"]
[null,null,3,"多向指示地贴",100,"40*120","地贴",null,"迪斯飞丝可移车贴不掉胶"]
[null,null,4,"区域地贴（等候区等）",20,"40*120","地贴",null,"迪斯飞丝可移车贴不掉胶"]
[null,null,5,"窗口标识",10,"30*100","8MM亚克力雕刻",null,"8MM压克力雕刻，钻石抛光，反面丝网印刷，"]
[null,null,6,"楼层索引标识",1,"50*220","落地不锈钢造型",null,"1.5MM304不锈钢激光切割，焊接造型，内部镀锌管焊接框架，精工打磨，表面汽车烤漆，内容5MM压克力丝网印刷，上下铝合金扣件，内容可更换,底座厚30CM，侧厚12CM"]
[null,null,7,"当前楼层科室指引标识",1,"40*80","不锈钢造型",null,"1.5MM304不锈钢激光切割，焊接造型，精工打磨，表面汽车烤漆，内容丝网印刷"]
[null,null,8,"通道吊牌",3,"150*30","不锈钢造型",null,"1.5MM304不锈钢激光切割，焊接造型，精工打磨，表面汽车烤漆，内容扣空贴透光压克力板,厚10CM"]
[null,null,9,"科室牌",12,"15*30","不锈钢牌",null,"1.5MM304不锈钢激光切割，焊接造型，精工打磨，表面汽车烤漆，内容丝网印刷,2CM厚度"]
[null,null,10,"科室制度牌",12,"60*90","海报框",null,"铝合金型材，厚度2cm可开启边框，可更换画面2CM厚"]
[null,null,11,"科室专家介绍及去向牌",12,"60*100","海报框",null,"铝合金型材，厚度2cm可开启边框，可更换画面"]
[null,null,12,"各科宣传标识、标语",12,"200*15","亚克力雕刻、雪弗板雕刻",null,"8MM雪弗板雕刻喷漆芬兰绿，面上贴3MM白色压克力"]
[null,null,13,"安全类警示牌",4,"15*40","亚克力UV",null,"5mm透明亚克力背UV背覆写真"]
[null,null,14,"消防类警示牌",2,"15*40","亚克力UV",null,"5mm透明亚克力背UV背覆写真"]
[null,null,15,"公共设施牌",13,"20*30","亚克力UV",null,"5mm透明亚克力背UV背覆写真"]
[null,null,16,"提示类标语、标牌",3,"15*40","亚克力UV",null,"5mm透明亚克力背UV背覆写真"]
[null,null,17,"桌面台牌",15,"30*25","磁吸亚克力桌牌（木底）",null,"可更换磁性亚克力桌牌+铜版纸打印"]
[null,"二楼",1,"指示地贴",3,"40*120","地贴",null,"迪斯飞丝可移车贴不掉胶"]
[null,null,2,"通道吊牌",2,"150*30","不锈钢造型",null,"1.5MM304不锈钢激光切割，焊接造型，精工打磨，表面汽车烤漆，内容扣空贴透光压克力板,厚10CM"]
[null,null,3,"病房牌",11,"30*15","不锈钢牌",null,"1.5MM304不锈钢激光切割，焊接造型，精工打磨，表面汽车烤漆，内容丝网印刷,2CM厚度"]
[null,null,4,"功能室门牌",16,"30*12","不锈钢牌",null,"1.5MM304不锈钢激光切割，焊接造型，精工打磨，表面汽车烤漆，内容丝网印刷,2CM厚度"]
[null,null,5,"当前楼层科室病房指引标识",1,"40*80","不锈钢造型",null,"1.5MM304不锈钢激光切割，焊接造型，精工打磨，表面汽车烤漆，内容丝网印刷,2CM厚度"]
[null,null,6,"安全类警示牌",4,"15*40","亚克力UV",null,"5mm透明亚克力背UV背覆写真"]
[null,null,7,"消防类警示牌",3,"40*15","亚克力UV",null,"5mm透明亚克力背UV背覆写真"]
[null,null,8,"公共设施牌",3,"20*30","亚克力UV",null,"5mm透明亚克力背UV背覆写真"]
[null,null,9,"安全提示类标语、标牌",3,"15*40","亚克力UV",null,"5mm透明亚克力背UV背覆写真"]
[null,null,10,"桌面台牌",15,"30*25","磁吸亚克力桌牌（木底）",null,"可更换磁性亚克力桌牌+铜版纸打印"]
[null,"三楼",1,"指示地贴",3,"40*120","地贴",null,"迪斯飞丝可移车贴不掉胶"]
[null,null,2,"通道吊牌",2,"150*30","不锈钢造型",null,"1.5MM304不锈钢激光切割，焊接造型，精工打磨，表面汽车烤漆，内容扣空贴透光压克力板,厚10CM"]
[null,null,3,"病房牌",11,"30*15","不锈钢牌",null,"1.5MM304不锈钢激光切割，焊接造型，精工打磨，表面汽车烤漆，内容丝网印刷,2CM厚度"]
[null,null,4,"功能室门牌",16,"30*12","不锈钢牌",null,"1.5MM304不锈钢激光切割，焊接造型，精工打磨，表面汽车烤漆，内容丝网印刷,2CM厚度"]
[null,null,5,"当前楼层科室病房指引标识",1,"40*80","不锈钢造型",null,"1.5MM304不锈钢激光切割，焊接造型，精工打磨，表面汽车烤漆，内容丝网印刷,2CM厚度"]
[null,null,6,"安全类警示牌",4,"15*40","亚克力UV",null,"5mm透明亚克力背UV背覆写真"]
[null,null,7,"消防类警示牌",2,"40*15","亚克力UV",null,"5mm透明亚克力背UV背覆写真"]
[null,null,8,"公共设施牌",2,"20*30","亚克力UV",null,"5mm透明亚克力背UV背覆写真"]
[null,null,9,"安全提示类标语、标牌",2,"15*40","亚克力UV",null,"5mm透明亚克力背UV背覆写真"]
[null,null,10,"桌面台牌",15,"30*25","磁吸亚克力桌牌（木底）",null,"可更换磁性亚克力桌牌+铜版纸打印"]
[null,"四楼",1,"指示地贴",3,"40*120","地贴",null,"迪斯飞丝可移车贴不掉胶"]
[null,null,2,"通道吊牌",2,"150*30","不锈钢造型",null,"1.5MM304不锈钢激光切割，焊接造型，精工打磨，表面汽车烤漆，内容扣空贴透光压克力板,厚10CM"]
[null,null,3,"病房牌",11,"30*15","不锈钢牌",null,"1.5MM304不锈钢激光切割，焊接造型，精工打磨，表面汽车烤漆，内容丝网印刷,2CM厚度"]
[null,null,4,"功能室门牌",12,"30*12","不锈钢牌",null,"1.5MM304不锈钢激光切割，焊接造型，精工打磨，表面汽车烤漆，内容丝网印刷,2CM厚度"]
[null,null,5,"当前楼层科室病房指引标识",1,"40*80","不锈钢造型",null,"1.5MM304不锈钢激光切割，焊接造型，精工打磨，表面汽车烤漆，内容丝网印刷,2CM厚度"]
[null,null,6,"安全类警示牌",4,"15*40","亚克力UV",null,"5mm透明亚克力背UV背覆写真"]
[null,null,7,"消防类警示牌",2,"40*15","亚克力UV",null,"5mm透明亚克力背UV背覆写真"]
[null,null,8,"公共设施牌",2,"20*30","亚克力UV",null,"5mm透明亚克力背UV背覆写真"]
[null,null,9,"安全提示类标语、标牌",2,"15*40","亚克力UV",null,"5mm透明亚克力背UV背覆写真"]
[null,null,10,"桌面台牌",15,"30*25","磁吸亚克力桌牌（木底）",null,"可更换磁性亚克力桌牌+铜版纸打印"]
[null,"五楼",1,"指示地贴",3,"40*120","地贴",null,"迪斯飞丝可移车贴不掉胶"]
[null,null,2,"通道吊牌",2,"150*30","不锈钢造型",null,"1.5MM304不锈钢激光切割，焊接造型，精工打磨，表面汽车烤漆，内容扣空贴透光压克力板,厚10CM"]
[null,null,3,"功能室门牌",20,"30*15","不锈钢牌",null,"1.5MM304不锈钢激光切割，焊接造型，精工打磨，表面汽车烤漆，内容丝网印刷,2CM厚度"]
[null,null,4,"当前楼层科室指引标识",1,"40*80","不锈钢造型",null,"1.5MM304不锈钢激光切割，焊接造型，精工打磨，表面汽车烤漆，内容丝网印刷,2CM厚度"]
[null,null,5,"安全类警示牌",4,"15*40","亚克力UV",null,"5mm透明亚克力背UV背覆写真"]
[null,null,6,"消防类警示牌",2,"40*15","亚克力UV",null,"5mm透明亚克力背UV背覆写真"]
[null,null,7,"公共设施牌",2,"20*30","亚克力UV",null,"5mm透明亚克力背UV背覆写真"]
[null,null,8,"安全提示类标语、标牌",2,"15*40","亚克力UV",null,"5mm透明亚克力背UV背覆写真"]
[null,null,9,"桌面台牌",44,"30*25","磁吸亚克力桌牌（木底）",null,"可更换磁性亚克力桌牌+铜版纸打印"]
[null,"显示屏",1,"显示屏",1,"60*650","LED显示屏",null,"LED单色12000点，黑色9.5cm型材，型号4590."]
[null,null,2,"显示屏","M2","300*220","LED显示屏",null,"P 2.5全彩显示屏，视频处理器，5V40A全彩电源，发送卡，接收卡，4590黑色型材边框，显示模组，物理16万点，不包含主电主网、控制电脑和配电柜"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}